**Small room fan ECA 100 ipro**

Standard model

On/off with light switch or separate switch.

Operation either at level 1 or 2.

Can be operated at two levels with standard double reversing switch.

Speed controllable.

Features

Intelligently programmed small room fan for very demanding requirements.

2 performance levels.

Designer cover conceals the inlet.

For air extraction.

VDE-GS symbol, exception: ECA 100 ipro RC / RCH

VDE mark: ECA 100 RC/RCH.

IP X5 degree of protection for safety in the bathroom.

Protection class II.

Suitable for continuous operation.

Thermal overload protection.

Colour: traffic white, similar to RAL 9016.

Housing made of impact resistant plastic material.

Motor

Energy-saving robust motor with ball bearings, maintenance-free.

Suitable for continuous operation.

Mounting information

Simplest installation as the cover can be removed with tools.

Wall and ceiling installation is possible.

Compatible with ECA predecessor models DN100, because screw holes and cable entry are in the same place.

Electrical connection

Recessed mounted electrical connection.

Safety instructions

All ECA 100 ipro units can be used in protection area 1 in accordance with DIN VDE 0100-701.

For details, please refer to the planning instructions.

Technical data

|  |  |
| --- | --- |
| Article: | ECA 100 ipro |
| Model: | Standard model |
| Air flow volume: | 78 m³/h / 92 m³/h |
| Rotating speed: | 2.100 1/min / 2.500 1/min |
| Speed controllable: |  ✔  |
| Reversing capacity: |  -  |
| SEC average: | -10,69 kWh/(m²\*a) |
| Type of voltage: | Alternating current |
| Rated voltage: | 230 V |
| Frequency: | 50 Hz |
| Nominal output: | 6 W / 8 W |
| Imax: | 0,06 A |
| Degree of protection: | IP X5 |
| Mains cable: | 3/5 x 1.5 mm² |
| Installation site: | Ceiling / Wall |
| Type of installation: | Surface-mounted |
| Installation position: | any |
| Material: | Synthetic material |
| Colour: | Traffic white, similar to RAL 9016 |
| Weight: | 0,7 kg |
| Weight including packaging: | 0,85 kg |
| Shutter: | none |
| Nominal size: | 100 mm |
| Width: | 159 mm |
| Height: | 159 mm |
| Depth: | 130 mm |
| Width with packaging: | 165 mm |
| Height with packaging: | 165 mm |
| Depth with packaging: | 145 mm |
| Airstream temperature at IMax: | 40 °C |
| Sound pressure level: | 27 dB(A) / 32 dB(A) Distance 3 m, Free-field conditions |
| Packing unit: | 1 piece |
| Range: | A |
| GTIN (EAN): | 4012799842002 |
| Article number: | 0084.0200 |

Manufacturer: MAICO

ECA 100 ipro Small room fan