**Internal shutter, electric AE 10/1**

Internal shutters for ventilation and air extraction.

Regulation of the basic ventilation through adjustable opening angle.

Heat energy saving by opening as required.

Control with commercially available circuit breakers, time switches and time delay relays.

Degree of protection IPX4.

Can be combined with the FE 100/1 window installation kit.

Technical data

|  |  |
| --- | --- |
| Article: | AE 10/1 |
| Air direction: | Ventilation and air extraction |
| Type of voltage: | Alternating current |
| Rated voltage: | 230 V |
| Frequency: | 50 Hz |
| Power consumption: | 5 W |
| Inom: | 25 mA |
| Degree of protection: | IP X4 |
| Mains cable: | 3 x 1,5 mm² |
| Installation: | Inside |
| Installation site: | Wall / Ceiling |
| Type of installation: | Surface-mounted |
| Installation position: | vertical / horizontal |
| Material: | Synthetic material |
| Colour: | Traffic white, similar to RAL 9016 |
| Weight: | 0,31 kg |
| Weight including packaging: | 0,42 kg |
| Type of shutter: | electrical |
| Nominal size: | 100 mm |
| Suitable for nominal size: | 100 mm |
| Width: | 159 mm |
| Height: | 159 mm |
| Depth: | 85 mm |
| Width with packaging: | 170 mm |
| Height with packaging: | 170 mm |
| Depth with packaging: | 110 mm |
| Ambient temperature: | 40 °C |
| Packing unit: | 1 piece |
| Range: | A |
| GTIN (EAN): | 4012799514008 |
| Article number: | 0151.0400 |

Manufacturer: MAICO

AE 10/1 Internal shutter, electric