**Additional circuit board ZP 2**

The ZP 2 additional circuit board is used to control optional components, e.g.

to realise the very useful function of pressure consistency for the DC fans

for differential pressure-controlled filter monitoring.

Communication between the basic PCB and additional board ZP 2 is established via the RJ 12 modular cable supplied.

The desired function can be selected via the Dip switch on the ZP 2.

With differential pressure controller integrated on the circuit board.

The pressure tubings are included in the scope of delivery.

For WS 120 Trio, WS 160 Flat, WS 170, WS 300 Flat, WR 310 / WR 410, WS 320 and WS 470 centralised ventilation units.

Technical data

|  |  |
| --- | --- |
| Article: | ZP 2 |
| Weight: | 0,06 kg |
| Weight including packaging: | 0,16 kg |
| Width: | 63 mm |
| Height: | 43 mm |
| Depth: | 79 mm |
| Width with packaging: | 173 mm |
| Height with packaging: | 79 mm |
| Depth with packaging: | 157 mm |
| Packing unit: | 1 piece |
| Suitable for products: | WS 160 Flat, WS 170 KB.., WS 320, WS 470, WR 310, WR 410 |
| Range: | K |
| GTIN (EAN): | 4012799925552 |
| Article number: | 0092.0555 |

Manufacturer: MAICO

ZP 2 Additional circuit board