**Sound-insulation distributor SDV 125/6-75**

Air distributor with integrated sound insulation.

Module for noise reduction of the supply or exhaust air flows of MAICO controlled domestic ventilation units.

1 duct connection on the unit side (Ø 125 mm) and 6 connections on the room side (Ø 75 mm).

Compatible with MAICOFlex and MAICOAir.

Technical data

|  |  |
| --- | --- |
| Article: | SDV 125/6-75 |
| Installation site: | Ceiling / Wall / Sloping roof |
| Material: | Sheet metal |
| Colour: | Silver |
| Weight: | 7,6 kg |
| Weight including packaging: | 9,8 kg |
| Number of couplings: | 6 |
| Nominal size: | 125 mm |
| Suitable for nominal size: | 75 mm |
| Width: | 298 mm |
| Height: | 215 mm |
| Depth: | 800 mm |
| Width with packaging: | 360 mm |
| Height with packaging: | 270 mm |
| Depth with packaging: | 890 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799926092 |
| Article number: | 0092.0609 |

Manufacturer: MAICO

SDV 125/6-75 Sound-insulation distributor