**Outgoing air wall connection KW-FL 12W**

The attractive stainless steel outgoing air wall supports are fitted on the outside wall of a building and are intended for blowing out outgoing air.

The outgoing air is blown out to the front.

An outgoing air cowl with condensate drip edge and bird protection grille is included in the scope of delivery.

Technical data

|  |  |
| --- | --- |
| Article: | KW-FL 12W |
| Air direction: | Air extraction |
| Installation site: | Outside wall |
| Material: | Stainless steel (V2A) |
| Colour: | Pure white, similar to RAL 9010 |
| Weight: | 1,16 kg |
| Weight including packaging: | 1,31 kg |
| Nominal size: | 125 mm |
| Width: | 172 mm |
| Height: | 203 mm |
| Depth: | 88 mm |
| Width with packaging: | 195 mm |
| Height with packaging: | 215 mm |
| Depth with packaging: | 185 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799520764 |
| Article number: | 0152.0076 |

Manufacturer: MAICO

KW-FL 12W Outgoing air wall connection