**harmful gas sensor SGS**

Anaesthetic gas, methane, propane and butane concentrations are permanently measured by a high-quality gas sensor.

If anaesthetic gas or gas is detected, an optical (red alarm indicator) and acoustic (loud signal horn) alarm is issued.

1A/30V DC relay output, potential-free contact, for triggering an output signal.

Technical data

|  |  |
| --- | --- |
| Article: | SGS |
| Rated voltage: | 12 V DC (-10% / +20%) |
| Imax: | 90 mA / 145 mA |
| Degree of protection: | IP 20 |
| Installation site: | WS units |
| Installation position: | any |
| Housing material: | Synthetic material |
| Colour: | White |
| Weight: | 0,22 kg |
| Weight including packaging: | 0,3 kg |
| Width: | 115 mm |
| Height: | 90 mm |
| Depth: | 30 mm |
| Width with packaging: | 165 mm |
| Height with packaging: | 150 mm |
| Depth with packaging: | 80 mm |
| Ambient temperature: | -10 °C up to 40 °C |
| Packing unit: | 1 piece |
| Suitable for products: | Trio, WS 160 Flat KET / KBET / KBZET, WS 170..., WS 300 Flat, WS 320..., WS 470... |
| Range: | K |
| GTIN (EAN): | 4012799992196 |
| Article number: | 0093.1323 |

Manufacturer: MAICO

SGS harmful gas sensor