**Flexible aluminium duct AFR 75**

Flexible five-layered, grooved aluminium duct to be used as connecting duct to the main duct, in accordance with DIN 18017-3.

Non-combustible in accordance with DIN 4102 class A1 (building material classification).

Length details: extended length.

Technical data

|  |  |
| --- | --- |
| Article: | AFR 75 |
| Max. operating pressure: | 2.500 Pa |
| Type of installation: | Recessed-mounted |
| Material: | Aluminium |
| Weight: | 0,37 kg |
| Weight including packaging: | 0,54 kg |
| Suitable for nominal size: | 75 mm |
| Length: | 3 m |
| Width: | 3.000 mm |
| Height: | 80 mm |
| Depth: | 80 mm |
| Width with packaging: | 810 mm |
| Height with packaging: | 100 mm |
| Depth with packaging: | 100 mm |
| Ambient temperature: | 100 °C |
| Packing unit: | 1 piece |
| Range: | B |
| GTIN (EAN): | 4012799550884 |
| Article number: | 0055.0088 |

Manufacturer: MAICO

AFR 75 Flexible aluminium duct