**Small room fan ECA 15/2 KF**

Technical data

|  |  |
| --- | --- |
| Article: | ECA 15/2 KF |
| Model: | Light control |
| Air flow volume: | 310 m³/h |
| Rotating speed: | 2.650 1/min |
| Speed controllable: | - |
| Type of voltage: | Alternating current |
| Rated voltage: | 230 V |
| Power consumption: | 45 W |
| Imax: | 0,28 A |
| Degree of protection: | IP 31 |
| Mains cable: | 2 x 1,5 mm² |
| Installation site: | Ceiling / Wall |
| Installation position: | any |
| Material: | Synthetic material |
| Colour: | Traffic white, similar to RAL 9016 |
| Weight: | 1,4 |
| Nominal size: | 150 mm |
| Sound pressure level: | 56 dB(A) |
| Packing unit: | 1 piece |
| Article number: | 0080.0978 |

Manufacturer: MAICO

ECA 15/2 KF Small room fan