**Protective grille, metal SG 40**

Protective grille for fans in accordance with DIN EN ISO 13857.

Suitable for fans with duct connections.

Can be fitted on the inlet or pressure side.

Made of antistatic material, for use in areas subject to explosion hazards.

Technical data

|  |  |
| --- | --- |
| Article: | SG 40 |
| Air direction: | Ventilation and air extraction |
| Material: | Wire, chromated |
| Weight: | 0,7 kg |
| Weight including packaging: | 0,7 kg |
| Suitable for nominal size: | 400 mm |
| Width: | 455 mm |
| Height: | 455 mm |
| Depth: | 5,5 mm |
| Width with packaging: | 455 mm |
| Height with packaging: | 455 mm |
| Depth with packaging: | 455 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799501183 |
| Article number: | 0150.0118 |

Manufacturer: MAICO

SG 40 Protective grille, metal