**Axial roof fan DZD 50/84 A**

Technical data

|  |  |
| --- | --- |
| Article: | DZD 50/84 A |
| Air flow volume: | 3.050 m³/h / 6.400 m³/h |
| Rotating speed: | 715 1/min / 1.425 1/min |
| Power consumption: | 160 W / 700 W |
| Imax: | 0,55 A / 1,6 A |
| Degree of protection: | IP 55 |
| Pole-changeable: | ✔ |
| Installation site: | Roof |
| Installation position: | vertical |
| Material: | Sheet steel, galvanised |
| Weight: | 37,5 |
| Packing unit: | 1 piece |
| Article number: | 0087.0449 |

Manufacturer: MAICO

DZD 50/84 A Axial roof fan