**Internal shutter MCV 30**

Internal shutters for air extraction and ventilation.

Manual activation with pull cord.

Parallel shutter blades.

Technical data

|  |  |
| --- | --- |
| Article: | MCV 30 |
| Air direction: | Ventilation / Air extraction |
| Max. flow velocity: | 2 m/s |
| Installation site: | Wall |
| Installation position: | vertical / horizontal |
| Material: | Sheet steel, stove-enamelled |
| Colour: | White |
| Lamella colour: | Black |
| Weight: | 3 |
| Type of shutter: | manual |
| Suitable for nominal size: | 300 mm |
| Open cross section: | 730 cm² |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799510536 |
| Article number: | 0151.0053 |

Manufacturer: MAICO

MCV 30 Internal shutter