**5-step transformer TRV 1,7-1**

5-step transformers for setting speed.

To control three-phase AC fans.

With motor protection switch.

With main contactor and control fuse.

With operating indicator light.

A shutter can be controlled via L2.

Technical data

|  |  |
| --- | --- |
| Article: | TRV 1,7-1 |
| Type of voltage: | Three-phase AC |
| Rated voltage: | 400 V |
| Frequency: | 50 Hz/60 Hz |
| Maximum load: | 1,7 A |
| Degree of protection: | IP 54 |
| Secondary voltage: | 105 V / 150 V / 190 V / 250 V / 400 V |
| Type of installation: | Surface-mounted |
| Housing material: | Synthetic material |
| Colour: | Light grey |
| Weight: | 9,3 kg |
| Weight including packaging: | 9,8 kg |
| Width: | 290 mm |
| Height: | 240 mm |
| Depth: | 190 mm |
| Width with packaging: | 340 mm |
| Height with packaging: | 240 mm |
| Depth with packaging: | 295 mm |
| Ambient temperature: | 0 °C up to 40 °C |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799575337 |
| Article number: | 0157.0533 |

Manufacturer: MAICO

TRV 1,7-1 5-step transformer