**Servomotor MS 8**

Servomotors for opening and closing the RKP duct shutter and JRE blind control shutter.

With limiting strap for torsion safety.

Can be combined with drive axis up to 20 mm diameter or 16 mm square.

Maximum turning angle: 90°.

Turning angle limit adjustable in 5° steps.

With two-point control for "Open" and "Closed" settings.

Drive axis can be rotated to the right or left.

MS 8 P: With 2 additional auxiliary switches.

Not suitable for use in areas subject to explosion hazards.

Installation instruction

With pushbutton for release of the gear, e.g. for manual setting of the shutter.

If PG 11 screws are used: IP 54 degree of protection.

Note: US 16 T universal contactor or customer-provided relay required for speed control with phase angles.

4-core mains cable is needed.

Technical data

|  |  |
| --- | --- |
| Article: | MS 8 |
| Type of voltage: | Alternating current |
| Rated voltage: | 230 V |
| Frequency: | 50 Hz/60 Hz |
| Maximum load (inductive load): | 2 A |
| Maximum load (ohmic load): | 10 A |
| Degree of protection: | IP 44 |
| Housing material: | Synthetic material, weather and UV resistant |
| Colour: | Blue |
| Weight: | 1,26 kg |
| Weight including packaging: | 1,32 kg |
| Width: | 100 mm |
| Height: | 180 mm |
| Depth: | 65 mm |
| Width with packaging: | 113 mm |
| Height with packaging: | 200 mm |
| Depth with packaging: | 80 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799577607 |
| Article number: | 0157.0760 |

Manufacturer: MAICO

MS 8 Servomotor