**Air filter, replacement FE 20-1**

Replacement filter for TFE...-4 air filter.

Technical data

|  |  |
| --- | --- |
| Article: | FE 20-1 |
| Installation position: | vertical / horizontal |
| Material: | Synthetic |
| Weight: | 0,47 kg |
| Weight including packaging: | 0,49 kg |
| Filter class: | ISO Coarse 70 % (G4) |
| Suitable for nominal size: | 200 mm |
| Width: | 340 mm |
| Height: | 270 mm |
| Depth: | 8 mm |
| Width with packaging: | 520 mm |
| Height with packaging: | 390 mm |
| Depth with packaging: | 50 mm |
| Ambient temperature: | 100 °C |
| Packing unit: | 2 pieces |
| Range: | C |
| GTIN (EAN): | 4012799990543 |
| Article number: | 0093.1225 |

Manufacturer: MAICO

FE 20-1 Air filter, replacement