**Fan insert ER 17/100 VZ**

Technical data

|  |  |
| --- | --- |
| Article: | ER 17/100 VZ |
| Model: | Time delay switch |
| Air flow volume: | 100 m³/h |
| Rotating speed: | 2.600 1/min |
| Speed controllable: |  -  |
| Rated voltage: | 230 V |
| Power consumption: | 68 W |
| Imax: | 0,4 A |
| Mains cable: | 3 x 1,5 mm² |
| Installation site: | Ceiling / Wall |
| Type of installation: | Recessed-mounted |
| Installation position: | any |
| Weight: | 2,4 |
| Nominal size: | 75 mm |
| Packing unit: | 1 piece |
| Article number: | 0080.0740 |

Manufacturer: MAICO

ER 17/100 VZ Fan insert