**Air filter TFE 10**

Air filter for ventilation systems.

Inspection lid can be removed for easy filter exchange.

With filter insert made of synthetic fibre.

Filter insert cannot be regenerated.

With rubber seal on the air connection couplings.

Accessories: Replacement air filter FE.. .

Recommended accessories: DW 1000 differential pressure controller.

Installation instructions

Monitor filter resistance using DW 1000 differential pressure controller.

Technical data

|  |  |
| --- | --- |
| Article: | TFE 10 |
| Housing material: | Sheet steel, galvanised |
| Weight: | 2,1 |
| Filter class: | G4 |
| Nominal size: | 100 mm |
| Ambient temperature: | 100 °C |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799490401 |
| Article number: | 0149.0040 |

Manufacturer: MAICO

TFE 10 Air filter