**Air filter ZFF 40**

Air filter for cleaning the fresh air supply.

With protection against accidental contact.

Simple filter replacement.

Accessories: Replacement air filter FF.. .

Technical data

|  |  |
| --- | --- |
| Article: | ZFF 40 |
| Installation: | Inside |
| Installation position: | vertical / horizontal |
| Material: | Synthetic material |
| Colour: | Pearl white, similar to RAL 1013 |
| Weight: | 2,44 kg |
| Weight including packaging: | 3,96 kg |
| Filter class: | ISO Coarse 30 % (G2) |
| Suitable for nominal size: | 350 mm / 400 mm |
| Width: | 470 mm |
| Height: | 470 mm |
| Depth: | 112 mm |
| Width with packaging: | 480 mm |
| Height with packaging: | 480 mm |
| Depth with packaging: | 130 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799490050 |
| Article number: | 0149.0005 |

Manufacturer: MAICO

ZFF 40 Air filter