**DZQ 40/126 A**

Technical data

|  |  |
| --- | --- |
| Article: | DZQ 40/126 A |
| Air flow volume: | 1.450 m³/h / 2.800 m³/h |
| Rotating speed: | 465 1/min / 930 1/min |
| Speed controllable: |  -  |
| Reversing capacity: |  -  |
| Power consumption: | 55 W / 150 W |
| Imax: | 0,2 A / 0,55 A |
| Pole-changeable: |  -  |
| Weight: | 10,2 |
| Airstream temperature at IMax: | 90 °C |
| Packing unit: | 1 piece |
| Article number: | 0083.0453 |

Manufacturer: MAICO

DZQ 40/126 A