**Axial ceiling fan EC 90 A**

Technical data

|  |  |
| --- | --- |
| Article: | EC 90 A |
| Maximum air circulation: | 11.000 m³/h |
| Rotating speed: | 420 1/min |
| Impeller diameter: | 900 mm |
| Power consumption: | 100 W |
| Imax: | 0,55 A |
| Degree of protection: | IP 55 |
| Installation site: | Ceiling |
| Weight: | 6,5 |
| Airstream temperature at nominal current: | 55 °C |
| Ambient temperature: | 55 °C |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799881209 |
| Article number: | 0088.0120 |

Manufacturer: MAICO

EC 90 A Axial ceiling fan