**5-step transformer TRV 1,0**

5-step transformers for setting speed.

To control three-phase AC fans.

With motor protection switch.

With main contactor and control fuse.

With operating indicator light.

A shutter can be controlled via L2.

Technical data

|  |  |
| --- | --- |
| Article: | TRV 1,0 |
| Maximum load: | 1 A |
| Housing material: | Synthetic material |
| Weight: | 5,98 |
| Weight including packaging: | 5,98 kg |
| Width: | 168 mm |
| Height: | 220 mm |
| Depth: | 174 mm |
| Width with packaging: | 220 mm |
| Height with packaging: | 210 mm |
| Depth with packaging: | 270 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799577157 |
| Article number: | 0157.0715 |

Manufacturer: MAICO

TRV 1,0 5-step transformer