**Heat recovery unit WRG20-2H**

Technical data

|  |  |
| --- | --- |
| Article: | WRG20-2H |
| Air flow volume: | 100 m³/h |
| Rotating speed: | 1.320 1/min |
| Speed controllable: |  -  |
| Rated voltage: | 230 V |
| Power consumption: | 35 W |
| Imax: | 0,2 A |
| Degree of protection: | IP 20 |
| Material: | Synthetic material |
| Colour: | Traffic white, similar to RAL 9016 |
| Weight: | 4,7 |
| Airstream temperature at IMax: | 40 °C |
| Heat recovery rate: | 50 % |
| Packing unit: | 1 piece |
| Article number: | 0082.0231 |

Manufacturer: MAICO

WRG20-2H Heat recovery unit