**DZQ 50/6 A**

Technical data

|  |  |
| --- | --- |
| Article: | DZQ 50/6 A |
| Air flow volume: | 5.700 m³/h |
| Rotating speed: | 930 1/min |
| Speed controllable: |  -  |
| Reversing capacity: |  -  |
| Power consumption: | 275 W |
| Imax: | 0,75 A |
| Degree of protection: | IP 55 |
| Pole-changeable: |  -  |
| Weight: | 19 |
| Airstream temperature at IMax: | 80 °C |
| Packing unit: | 1 piece |
| Article number: | 0083.0430 |

Manufacturer: MAICO

DZQ 50/6 A