**Air filter, replacement FE 31-2**

Replacement filter for TFE...-4 air filter.

Technical data

|  |  |
| --- | --- |
| Article: | FE 31-2 |
| Installation position: | vertical / horizontal |
| Material: | Synthetic |
| Weight: | 0,48 kg |
| Weight including packaging: | 0,5 kg |
| Filter class: | ISO Coarse 70 % (G4) |
| Suitable for nominal size: | 315 mm |
| Width: | 520 mm |
| Height: | 390 mm |
| Depth: | 6 mm |
| Width with packaging: | 521 mm |
| Height with packaging: | 391 mm |
| Depth with packaging: | 40 mm |
| Ambient temperature: | 100 °C |
| Packing unit: | 2 pieces |
| Range: | C |
| GTIN (EAN): | 4012799990567 |
| Article number: | 0093.1227 |

Manufacturer: MAICO

FE 31-2 Air filter, replacement