**Air filter TFE 12-4**

Air filter for ventilation systems.

Inspection lid can be removed for easy filter exchange.

With filter insert made of synthetic fibre.

Filter insert cannot be regenerated.

With rubber seal on the air connection couplings.

Accessories: Replacement air filter FE.. .

Recommended accessories: DW 1000 differential pressure controller.

Installation instructions

Monitor filter resistance using DW 1000 differential pressure controller.

Technical data

|  |  |
| --- | --- |
| Article: | TFE 12-4 |
| Installation position: | vertical / horizontal |
| Housing material: | Sheet steel, galvanised |
| Weight: | 2 kg |
| Weight including packaging: | 2,19 kg |
| Filter class: | ISO Coarse 70 % (G4) |
| Nominal size: | 125 mm |
| Width: | 210 mm |
| Height: | 200 mm |
| Depth: | 190 mm |
| Width with packaging: | 275 mm |
| Height with packaging: | 250 mm |
| Depth with packaging: | 220 mm |
| Ambient temperature: | 100 °C |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799490753 |
| Article number: | 0149.0075 |

Manufacturer: MAICO

TFE 12-4 Air filter