**Protective grille SGR 31**

Protective grille for fans in accordance with DIN EN ISO 13857.

Suitable for fans with duct connections.

Can be fitted on the inlet or pressure side.

Technical data

|  |  |
| --- | --- |
| Article: | SGR 31 |
| Air direction: | Ventilation and air extraction |
| Material: | Wire, chromated |
| Weight: | 0,48 kg |
| Weight including packaging: | 0,48 kg |
| Suitable for nominal size: | 315 mm |
| Width: | 315 mm |
| Height: | 315 mm |
| Depth: | 320 mm |
| Width with packaging: | 315 mm |
| Height with packaging: | 315 mm |
| Depth with packaging: | 320 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799501282 |
| Article number: | 0150.0128 |

Manufacturer: MAICO

SGR 31 Protective grille