**Brine pump controller EW-S**

Automatically controls summer and winter operation.

No seasonal operation required.

With fault display.

Switches the pump on at regular intervals, to avoid sticking.

With predefined factory settings.

With 2 temperature sensors for outside air temperature before and after the water-air heat exchanger.

Technical data

|  |  |
| --- | --- |
| Article: | EW-S |
| Weight: | 0,4 kg |
| Weight including packaging: | 0,565 kg |
| Width: | 160 mm |
| Height: | 110 mm |
| Depth: | 60 mm |
| Width with packaging: | 230 mm |
| Height with packaging: | 130 mm |
| Depth with packaging: | 185 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799572039 |
| Article number: | 0157.0203 |

Manufacturer: MAICO

EW-S Brine pump controller