**Power board DTL 2 P-L**

Additional board for installation in the DTL 24 P electronic temperature control to meet a power requirement of 16.5 kW to 30 kW.

Technical data

|  |  |
| --- | --- |
| Article: | DTL 2 P-L |
| Type of voltage: | Three-phase AC |
| Rated voltage: | 400 V |
| Weight: | 0,03 kg |
| Weight including packaging: | 0,04 kg |
| Width: | 60 mm |
| Height: | 35 mm |
| Depth: | 30 mm |
| Width with packaging: | 70 mm |
| Height with packaging: | 70 mm |
| Depth with packaging: | 40 mm |
| Packing unit: | 1 piece |
| Range: | D |
| GTIN (EAN): | 4012799575870 |
| Article number: | 0157.0587 |

Manufacturer: MAICO

DTL 2 P-L Power board