**Axial roof fan DZD30-2A**

Technical data

|  |  |
| --- | --- |
| Article: | DZD30-2A |
| Air flow volume: | 2.900 m³/h |
| Rotating speed: | 2.850 1/min |
| Power consumption: | 400 W |
| Imax: | 0,9 A |
| Degree of protection: | IP 55 |
| Pole-changeable: | - |
| Installation site: | Roof |
| Installation position: | vertical |
| Material: | Sheet steel, galvanised |
| Weight: | 17,8 |
| Packing unit: | 1 piece |
| Article number: | 0087.0416 |

Manufacturer: MAICO

DZD30-2A Axial roof fan