**Supplementary heating WS 75 NH**

Optional supplementary heat register for heating the supply air when outside temperatures are cold.

Technical data

|  |  |
| --- | --- |
| Article: | WS 75 NH |
| Rated voltage: | 230 VAC |
| Frequency: | 50 Hz |
| Nominal output: | 200 W |
| Degree of protection: | IP 00 |
| Material: | Aluminium/galvanised sheet steel |
| Colour: | Silver |
| Weight: | 0,6 kg |
| Weight including packaging: | 0,8 kg |
| Width: | 296 mm |
| Height: | 51 mm |
| Depth: | 106 mm |
| Width with packaging: | 315 mm |
| Height with packaging: | 125 mm |
| Depth with packaging: | 245 mm |
| Heater power rating: | 250 W |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799992431 |
| Article number: | 0093.1586 |

Manufacturer: MAICO

WS 75 NH Supplementary heating