**DZQ 40/2 A**

Technical data

|  |  |
| --- | --- |
| Article: | DZQ 40/2 A |
| Air flow volume: | 9.500 m³/h |
| Rotating speed: | 2.850 1/min |
| Speed controllable: | - |
| Reversing capacity: | - |
| Power consumption: | 2.000 W |
| Imax: | 3,5 A |
| Degree of protection: | IP 55 |
| Pole-changeable: | - |
| Weight: | 23 |
| Packing unit: | 1 piece |
| Article number: | 0083.0428 |

Manufacturer: MAICO

DZQ 40/2 A