**ECA 11 E 24 V**

Technical data

|  |  |
| --- | --- |
| Article: | ECA 11 E 24 V |
| Model: | Safety extra-low voltage (SELV) |
| Air flow volume: | 105 m³/h |
| Rotating speed: | 2.500 1/min |
| Speed controllable: | - |
| Type of voltage: | Alternating current |
| Rated voltage: | 24 V |
| Frequency: | 60 Hz |
| Power consumption: | 14 W |
| Imax: | 0,9 A |
| Degree of protection: | IP 45 |
| Type of installation: | Recessed-mounted |
| Installation position: | vertical / horizontal |
| Material: | Synthetic material |
| Colour: | Traffic white, similar to RAL 9016 |
| Weight: | 0,725 |
| Nominal size: | 100 mm |
| Sound pressure level: | 47 dB(A) |
| Packing unit: | 1 piece |
| Range: | A |
| GTIN (EAN): | 4012799804611 |
| Article number: | 0080.0461 |

Manufacturer: MAICO

ECA 11 E 24 V