**Outgoing air wall connection KW-FL 20W**

The attractive stainless steel outgoing air wall supports are fitted on the outside wall of a building and are intended for blowing out outgoing air.

The outgoing air is blown out to the front.

An outgoing air cowl with condensate drip edge and bird protection grille is included in the scope of delivery.

Technical data

|  |  |
| --- | --- |
| Article: | KW-FL 20W |
| Air direction: | Air extraction |
| Installation site: | Outside wall |
| Material: | Stainless steel (V2A) |
| Colour: | Pure white, similar to RAL 9010 |
| Weight: | 2,36 kg |
| Weight including packaging: | 2,64 kg |
| Nominal size: | 200 mm |
| Width: | 280 mm |
| Height: | 292 mm |
| Depth: | 126 mm |
| Width with packaging: | 315 mm |
| Height with packaging: | 300 mm |
| Depth with packaging: | 245 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799520849 |
| Article number: | 0152.0084 |

Manufacturer: MAICO

KW-FL 20W Outgoing air wall connection