**15° Drawn elbow, with O-ring gasket B15-180**

Technical data

|  |  |
| --- | --- |
| Article: | B15-180 |
| Type of installation: | Recessed-mounted |
| Ambient temperature: | 60 °C |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799553434 |
| Article number: | 0055.0343 |

Manufacturer: MAICO

B15-180 15° Drawn elbow, with O-ring gasket