**Thermostat THR 10**

Thermostat for controlling fans depending on the air temperature.

With automatic change over for summer / winter operation.

An US 16 T universal contactor is required for switching the three-phase AC fans.

Technical data

|  |  |
| --- | --- |
| Article: | THR 10 |
| Type of voltage: | Alternating current |
| Rated voltage: | 230 V |
| Maximum load (inductive load): | 2 A |
| Maximum load (ohmic load): | 10 A |
| Degree of protection: | IP 30 |
| Type of installation: | Surface-mounted |
| Colour: | Pearl white, similar to RAL 1013 |
| Weight: | 0,11 kg |
| Weight including packaging: | 0,14 kg |
| Width: | 76 mm |
| Height: | 82 mm |
| Depth: | 38 mm |
| Width with packaging: | 80 mm |
| Height with packaging: | 83 mm |
| Depth with packaging: | 45 mm |
| Temperature setting range: | 10 °C up to 30 °C |
| Differential gap: | approx. 1 K |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799577744 |
| Article number: | 0157.0774 |

Manufacturer: MAICO

THR 10 Thermostat