**External grille LZP-R 56**

Weather protection grille for ventilation and air extraction constructed to very high quality standard.

With channel cross-section extension as standard to reduce pressure losses.

With fixed rain-repellent weather protection lamella.

With frame for mounting in masonry walls.

With 20 mm flange frame and slots for direct connection with channel.

Protective grille in accordance with DIN EN ISO 13857.

Technical data

|  |  |
| --- | --- |
| Article: | LZP-R 56 |
| Air direction: | Ventilation and air extraction |
| Installation: | outside |
| Installation site: | Wall / Channel |
| Material: | Sheet steel, galvanised |
| Weight: | 31,5 kg |
| Weight including packaging: | 33,84 kg |
| Channel dimension: | 1.000 mm x 500 mm |
| Open cross section: | 4.050 cm² |
| Width: | 1.529 mm |
| Height: | 575 mm |
| Depth: | 73 mm |
| Width with packaging: | 1.575 mm |
| Height with packaging: | 575 mm |
| Depth with packaging: | 265 mm |
| Packing unit: | 1 piece |
| Range: | D |
| GTIN (EAN): | 4012799513872 |
| Article number: | 0151.0387 |

Manufacturer: MAICO

LZP-R 56 External grille