**45° Exhaust socket with O-ring gasket and protective grille ASR 80**

Technical data

|  |  |
| --- | --- |
| Article: | ASR 80 |
| Type of installation: | Recessed-mounted |
| Ambient temperature: | 60 °C |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799555230 |
| Article number: | 0055.0523 |

Manufacturer: MAICO

ASR 80 45° Exhaust socket with O-ring gasket and protective grille