**40 mm channel sound absorbers with lining and attenuating linging KSDA55/110/1200**

Features

40 mm channel sound absorbers with lining and silencer, collar size. Surface: Sendzimir galvanised.

Technical data

|  |  |
| --- | --- |
| Article: | KSDA55/110/1200 |
| Housing material: | Sheet steel, Sendzimir galvanised |
| Weight including packaging: | 0 kg |
| Channel dimension: | 110 mm x Array x 55 mm |
| Width: | 260 mm |
| Width with packaging: | 0 mm |
| Height with packaging: | 0 mm |
| Depth with packaging: | 0 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799924708 |
| Article number: | 0092.0470 |

Manufacturer: MAICO

KSDA55/110/1200 40 mm channel sound absorbers with lining and attenuating linging