**Air filter, replacement WSF-AKF 170**

Replacement air filters for WS 160 Flat and WS 170... centralised ventilation units

All WS 160 Flat and WS 170... units can be equipped in the outside air with an ISO Coarse 80 % (G4) / ISO ePM1 55 % (F7) filter combination.

Alternative to the ISO ePM1 55 % (F7) filter, the ISO ePM10 80 % (M5) active carbon filter.

Technical data

|  |  |
| --- | --- |
| Article: | WSF-AKF 170 |
| Installation position: | vertical / horizontal |
| Weight: | 0,26 kg |
| Weight including packaging: | 0,27 kg |
| Type of filter: | Active charcoal filter |
| Filter class: | ISO ePM10 80 % (M5) |
| Width: | 400 mm |
| Height: | 173 mm |
| Depth: | 50 mm |
| Width with packaging: | 402 mm |
| Height with packaging: | 175 mm |
| Depth with packaging: | 52 mm |
| Packing unit: | 1 piece |
| Suitable for products: | WS 160 Flat, WS 170... |
| Range: | K |
| GTIN (EAN): | 4012799932727 |
| Article number: | 0093.0272 |

Manufacturer: MAICO

WSF-AKF 170 Air filter, replacement