**Axial roof fan DZD50-6A**

Technical data

|  |  |
| --- | --- |
| Article: | DZD50-6A |
| Air flow volume: | 4.000 m³/h |
| Rotating speed: | 930 1/min |
| Power consumption: | 220 W |
| Imax: | 0,65 A |
| Degree of protection: | IP 55 |
| Pole-changeable: | - |
| Installation site: | Roof |
| Installation position: | vertical |
| Material: | Sheet steel, galvanised |
| Weight: | 32,4 |
| Packing unit: | 1 piece |
| Article number: | 0087.00425 |

Manufacturer: MAICO

DZD50-6A Axial roof fan