**Fan insert ER 60 GVZC EC**

Model with EC motor, base load circuit and time delay

The unit runs in continuous operation at 35 m3/h.

Switching to full load with adjustable start delay (0/0.5/1/2/3 minutes).

Adjustable overrun time of the full load level (0/1/3/6/15 minutes).

Not speed-controllable.

Switching variation: The base load can be switched on or off by an additional switch (see the wiring diagrams online).

Features

Fan with cover and ISO Coarse > 30 % (G2) filter for installation in flush-mounted housing.

For single or second room air extraction using a single fan (exception: H model).

Trouble-free filter change without tools.

It is possible to rotate the cover by ± 5°, to compensate for housings which have been fitted at an angle.

Simple and quick installation of the fan in the housing via the snap-on attachment and the electrical plug connector.

Colour: traffic white, similar to RAL 9016.

All MAICO ER units have an IP X5 degree of protection and can be installed in area 1 in accordance with DIN VDE 0100-701, even with water jets. For details see planning instructions.

Protection class II.

The extremely steep characteristic curve shows the high pressure capacity of the ER fans.

Robust energy-saving capacitor motor.

Motor with thermal overload protection.

Maintenance-free, with enclosed ball bearings on both sides.

Volumetric flow characteristic curve and air leakage rate checked by TÜV Bayern e.V (German Technical Inspection Agency). Air leakage rate < 0.01 m³/h.

Shaft level difference according to DIN 4109, tested by IAB Oberursel (The Institute for Acoustics and Building Physics in Germany).

With VDE symbol.

Technical data

|  |  |
| --- | --- |
| Article: | ER 60 GVZC EC |
| Model: | EC model with base load and time delay switching. |
| Air flow volume: | 35 m³/h / 62 m³/h |
| Rotating speed: | 850 1/min / 1.250 1/min |
| Speed controllable: | - |
| SEC average: | -12,77 kWh/(m²\*a) |
| Type of voltage: | Alternating current |
| Rated voltage: | 230 V |
| Frequency: | 50 Hz |
| Power consumption: | 3,9 W / 6 W |
| Imax: | 0,03 A / 0,05 A |
| Degree of protection: | IP X5 |
| Mains cable: | 5 x 1,5 mm² |
| Type of installation: | Recessed-mounted |
| System type: | Decentralised |
| Material: | Synthetic material |
| Colour: | Traffic white, similar to RAL 9016 |
| Weight: | 1,7 kg |
| Weight including packaging: | 1,506 kg |
| Filter class: | ISO Coarse 30 % (G2) |
| Air outlet direction: | at side |
| Width: | 280 mm |
| Height: | 280 mm |
| Depth: | 160 mm |
| Width with packaging: | 250 mm |
| Height with packaging: | 135 mm |
| Depth with packaging: | 250 mm |
| Airstream temperature at IMax: | 40 °C |
| Overrun time: | 0 min / 1 min / 3 min / 6 min / 15 min |
| Start delay: | 0 min / 0,5 min / 1 min / 2 min / 3 min |
| Packing unit: | 1 piece |
| Range: | B |
| GTIN (EAN): | 4012799841166 |
| Article number: | 0084.0116 |

Manufacturer: MAICO

ER 60 GVZC EC Fan insert