**Control shutter JRE 30**

Blind control shutters for automatic activation.

Must be combined with additional MS 8 or MS 8 P servomotors (servomotor is not included in the scope of delivery).

Do not use in areas subject to explosions.

Installation instructions

Ensure access to the servomotor.

Technical data

|  |  |
| --- | --- |
| Article: | JRE 30 |
| Air direction: | Ventilation and air extraction |
| Installation site: | Duct |
| Installation position: | vertical / horizontal |
| Material: | Sheet steel, galvanised |
| Weight: | 4,6 kg |
| Weight including packaging: | 4,9 kg |
| Type of shutter: | electrical |
| Suitable for nominal size: | 300 mm |
| Width: | 360 mm |
| Height: | 385 mm |
| Depth: | 165 mm |
| Width with packaging: | 420 mm |
| Height with packaging: | 405 mm |
| Depth with packaging: | 185 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799513919 |
| Article number: | 0151.0391 |

Manufacturer: MAICO

JRE 30 Control shutter