**External grille MGR 80/125 V2A**

MGR: External grille for covering round ventilation openings.

MGE: External grille for covering square ventilation openings.

With insect grille and spring-holder.

For duct diameters from 80 mm to 125 mm.

Technical data

|  |  |
| --- | --- |
| Article: | MGR 80/125 V2A |
| Model: | round |
| Air direction: | Air extraction |
| Material: | Stainless steel |
| Weight: | 0,1 kg |
| Weight including packaging: | 0,11 kg |
| External diameter: | 130 mm |
| Width: | 130 mm |
| Height: | 130 mm |
| Depth: | 130 mm |
| Width with packaging: | 130 mm |
| Height with packaging: | 27 mm |
| Depth with packaging: | 130 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799780342 |
| Article number: | 0078.0034 |

Manufacturer: MAICO

MGR 80/125 V2A External grille