**5-step transformer TRE 3,3-2**

5-step transformers for setting speed.

To control AC fans.

With operating indicator light.

Additional switching contact (230 V) e.g. for controlling a shutter.

Technical data

|  |  |
| --- | --- |
| Article: | TRE 3,3-2 |
| Type of voltage: | Alternating current |
| Rated voltage: | 230 V |
| Frequency: | 50 Hz/60 Hz |
| Nominal output: | 594 W |
| Maximum load: | 3,3 A |
| Degree of protection: | IP 54 |
| Secondary voltage: | 85 V / 115 V / 150 V / 180 V / 230 V |
| Type of installation: | Surface-mounted |
| Housing material: | Synthetic material |
| Colour: | Light grey, similar to RAL 7035 |
| Weight: | 3,86 kg |
| Weight including packaging: | 4,38 kg |
| Width: | 195 mm |
| Height: | 148 mm |
| Depth: | 175 mm |
| Width with packaging: | 235 mm |
| Height with packaging: | 235 mm |
| Depth with packaging: | 195 mm |
| Ambient temperature: | 0 °C up to 40 °C |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799571599 |
| Article number: | 0157.0159 |

Manufacturer: MAICO

TRE 3,3-2 5-step transformer