**5-step transformer, control cabinet TR 6,6 S-2**

5-step transformers for setting speed.

To control three-phase AC fans.

With foot bracket and connection terminals.

With profile rail for integral transformers < 3 kg.

Accessories: DSS 20 5-step switch.

Technical data

|  |  |
| --- | --- |
| Article: | TR 6,6 S-2 |
| Type of voltage: | Three-phase AC |
| Rated voltage: | 400 V |
| Frequency: | 50 Hz/60 Hz |
| Nominal output: | 1.188 W |
| Maximum load: | 6,6 A |
| Degree of protection: | IP 00 |
| Secondary voltage: | 105 V / 150 V / 190 V / 250 V / 400 V |
| Type of installation: | Control cabinet |
| Weight: | 20,02 kg |
| Weight including packaging: | 23,35 kg |
| Width: | 150 mm |
| Height: | 115 mm |
| Depth: | 155 mm |
| Width with packaging: | 310 mm |
| Height with packaging: | 420 mm |
| Depth with packaging: | 340 mm |
| Ambient temperature: | 0 °C up to 40 °C |
| Packing unit: | 2 pieces |
| Range: | C |
| GTIN (EAN): | 4012799571537 |
| Article number: | 0157.0153 |

Manufacturer: MAICO

TR 6,6 S-2 5-step transformer, control cabinet