**Outgoing air wall connection KW-FL 16E**

The attractive stainless steel outgoing air wall supports are fitted on the outside wall of a building and are intended for blowing out outgoing air.

The outgoing air is blown out to the front.

An outgoing air cowl with condensate drip edge and bird protection grille is included in the scope of delivery.

Technical data

|  |  |
| --- | --- |
| Article: | KW-FL 16E |
| Air direction: | Air extraction |
| Installation site: | Outside wall |
| Material: | Stainless steel (V2A) |
| Colour: | Stainless steel, brushed |
| Weight: | 1,57 kg |
| Weight including packaging: | 1,78 kg |
| Nominal size: | 160 mm |
| Width: | 220 mm |
| Height: | 232 mm |
| Depth: | 100 mm |
| Width with packaging: | 235 mm |
| Height with packaging: | 250 mm |
| Depth with packaging: | 210 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799520795 |
| Article number: | 0152.0079 |

Manufacturer: MAICO

KW-FL 16E Outgoing air wall connection