**Air filter TFP 28-7**

Air filter for ventilation systems.

Flanges on both sides for installation in square ventilation channels.

Inspection lid can be removed for easy filter exchange.

Accessories: KF.. replacement air filter and DW 1000 differential pressure controller.

Installation instructions

Mount the air filter on the fan's suction side.

Monitor filter resistance using DW 1000 differential pressure controller.

Provide sufficient space on the side for opening the inspection lid during a filter change.

Technical data

|  |  |
| --- | --- |
| Article: | TFP 28-7 |
| Installation site: | Channel |
| Installation position: | vertical / horizontal |
| Housing material: | Sheet steel, galvanised |
| Weight: | 11,2 kg |
| Weight including packaging: | 11,22 kg |
| Type of filter: | Dust and pollen filter |
| Filter class: | ISO ePM1 80 % (F7) |
| Channel dimension: | 600 mm x 300 mm |
| Width: | 640 mm |
| Height: | 340 mm |
| Depth: | 550 mm |
| Width with packaging: | 640 mm |
| Height with packaging: | 340 mm |
| Depth with packaging: | 550 mm |
| Airstream temperature at IMax: | 70 °C |
| Packing unit: | 1 piece |
| Range: | D |
| GTIN (EAN): | 4012799490692 |
| Article number: | 0149.0069 |

Manufacturer: MAICO

TFP 28-7 Air filter