**Window installation kit FE 100/1 AP**

Features

For the installation of small room fans of the ECA 100 ipro group in windows and thin walls.

Colour: traffic white, similar to RAL 9016.

Housing made of impact-resistant plastic.

Scope of delivery: AP shutter and/or SG external grille, 3 x spacing frames, 2 x gaskets, threaded connector, 3 x screws for fastening fan, tension relief bar with 2 x screws, cable grommet, installation instructions.

Mounting information

Easy assembly in window cut-out by adaptor which can be screwed into the threaded connector.

Pane thickness at least 3 mm, pane spacing up to 75 mm.

Window cut-out of 115 up to 120 mm.

Not suited for installation in double-glazed windows that can be swung open.

Electrical connection

On terminal block in housing of ECA 100 ipro...

Technical data

|  |  |
| --- | --- |
| Article: | FE 100/1 AP |
| Installation site: | Window / Thin wall |
| Installation position: | horizontal |
| Material: | Synthetic material, shock-resistant |
| Colour: | Traffic white, similar to RAL 9016 |
| Weight: | 0,4 kg |
| Weight including packaging: | 0,48 kg |
| Width: | 150 mm |
| Height: | 150 mm |
| Depth: | 103 mm |
| Width with packaging: | 157 mm |
| Height with packaging: | 157 mm |
| Depth with packaging: | 123 mm |
| Packing unit: | 1 piece |
| Range: | A |
| GTIN (EAN): | 4012799934998 |
| Article number: | 0093.0499 |

Manufacturer: MAICO

FE 100/1 AP Window installation kit