**Brine-air heat exchanger EW-K 160**

Brine-air heat exchanger for transferring the warmth from the brine to the outside air.

Condensation drainage with 1/2" connection on the side.

The connection between the register and the PE duct is done by the customer.

Technical data

|  |  |
| --- | --- |
| Article: | EW-K 160 |
| Max. volumetric flow: | 165 m³/h |
| Weight including packaging: | 6,85 kg |
| Brine connection nominal size: | 10 mm |
| Nominal size: | 160 mm |
| Width with packaging: | 380 mm |
| Height with packaging: | 285 mm |
| Depth with packaging: | 340 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799924043 |
| Article number: | 0192.0404 |

Manufacturer: MAICO

EW-K 160 Brine-air heat exchanger