**Glycosol N EW-G**

Heat carrying medium for transferring soil warmth to the outside air.

20 litre canister with 100 % Glykosol, sufficient for 100 m EW-D pressure duct at approx. 200 m³/h volumetric flow.

25 % Glykosol-water mixture in the duct circuit.

1 canister is enough to fill the circuit up completely.

Technical data

|  |  |
| --- | --- |
| Article: | EW-G |
| Weight: | 20 kg |
| Weight including packaging: | 21,4 kg |
| Width: | 300 mm |
| Height: | 250 mm |
| Depth: | 380 mm |
| Width with packaging: | 290 mm |
| Height with packaging: | 240 mm |
| Depth with packaging: | 270 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799310112 |
| Article number: | 0331.0011 |

Manufacturer: MAICO

EW-G Glycosol N