**Pressure duct EW-D**

PE high-pressure duct for EW brine geothermal heat exchanger.

Sufficient for approx. 200 m³/h volumetric flow.

Technical data

|  |  |
| --- | --- |
| Article: | EW-D |
| Max. operating pressure: | 12,5 bar |
| Weight: | 29 kg |
| Weight including packaging: | 29 kg |
| External diameter: | 32 mm |
| Width: | 1.150 mm |
| Height: | 1.150 mm |
| Depth: | 200 mm |
| Width with packaging: | 1.150 mm |
| Height with packaging: | 1.150 mm |
| Depth with packaging: | 200 mm |
| Wall thickness: | 2,9 mm |
| Packing unit: | 100 m |
| Range: | K |
| GTIN (EAN): | 4012799592006 |
| Article number: | 0059.0200 |

Manufacturer: MAICO

EW-D Pressure duct